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Note:
1. Ring flanges available overbored or counterbored per customer specification.2. Bolt holes shall be drilled 1/8th inch larger in diameter than the nominal diameter of the bolt, except for flanges larger than 84 inch in diameter which shall be drilled 3/16th inch larger than the nominal diameter of the bolt.3. Drilling same as ANSI/ASME B16.1 125 lb and B16.5 150 lb pattern.4. Flanges available overdrilled to accommodate insulators.5. AWWA recommends the use of dished head assemblies as alternate to blind flanges, sizes over 72" nominal.6. AWWA C207-01 Class B and D Hub Flanges are identical to Industry Standard Class 125 Light Weight Flanges.
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AWWA C207 - 01 D - Ring Flange
Pressure Rating at Atmospheric Temperature:

412175 PS.1. 14" & larger 150 P.S.
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