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High Frequency Longitudinal Seam Welded Steel Pipe is also called ERW steel pipes, is the abbreviation of Electric Resistance Welded steel pipes. It is pipe produced by heating the steel grade edges to melt by high frequency electric current and form a seam under pressure of rolls without filler metal.
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